Coupler tube is Wildman 3” FWFG

Use CAD files to 3D Print needed parts

Adjust all CAD files as needed and trim / sand / machine parts to obtain a good fit

Glue six 4-40 nuts to the underside of the flange

Screws are temporarily used to hold the nuts in place while the epoxy cures